
Firmware V1.0.32_AS.1

Applied for following Asoni models:
-----------------------------------------------
CAM613M
CAM614
CAM615
CAM616M
CAM619M
CAM620
CAM624M
CAM627M
CAM628M
CAM629
CAM634M
CAM635
CAM636M
CAM637M
CAM638
CAM639
CAM640
CAM641
CAM642M
CAM643
CAM646M
CAM649M
SVR610


Firmware Change Logs:
-------------------------------
V1.0.32
        1. Fix the following bug:
            When the recorded file in SD card over than page-3277, the camera stop to write into SD card.


V1.0.28
        1. Add supports "Save to Samba network disk" function.
        2. Add supports new H.264 camera models.
        3. Add provides "3 FPS" setting in "Frame Rate per Second" section in "Video Format" page.
        4. Add "Enable/Disable RTSP connection" option in "Network Setting" page.
        5. Add "Onvif" section in "Network Setting" page, user can select the Onvif standard (Onvif V1.01 and Onvif V1.02) for connection.
        6. Fix the following bug:
            When connecting to NVR6-series or SOL6-series recording software, after a period, the video becomes slow and lag.


V1.0.24
        1. Fix the following bug:
            After reboot camera, some parameters will be lost.


V1.0.22
        1. Add supports "Multicast" function.
        2. Add supports new H.264 camera models.
        3. Complaint with ONVIF V1.01 standard.
        4. Passed with "ONVIF V1.01 test tool". (SVR610 does not support ONVIF. If you want to test the other cameras with "ONVIF test tool", please set "Time to Reboot(ms)" to "60000")

